
[image: image1.png]


[image: image2.png]


[image: image3.jpg]


[image: image4.jpg]


[image: image5.png]D




[image: image6.png]



[image: image7.jpg]


[image: image8.png]o &

[ #




[image: image9.png]


[image: image10.png]


[image: image11.png]E ¥

| a2
o<
W



[image: image12.jpg]


[image: image13.jpg]


[image: image14.jpg]




[image: image15.png]


[image: image16.emf][image: image17.png]


[image: image18.png]



	Model
	XL-S-750

	Internal Dimension (mm)
	950*950*850 mm

	Overall Dimension (mm)
	1300*1420*1800 mm

	Specimen Holder Size(mm)
	95*200

	Specimen Capacity
	42pcs

	Chamber Type
	Rotating Holder

	Irradiation Source
	1 piece of 4500w water-cooled xenon arc lamp with inner quartz and outer borosilicate filter

	Parameter
	Irradiance Range
	35~150 W/㎡

	
	Bandwidth Measurement
	300nm~400nm (340nm or 420nm)

	
	Chamber Temperature Range
	Ambient ～ 100 ℃ ±2℃

	
	Black Panel Temperature
	BPT 35 ～ 85 ℃ ±2℃

	
	 Humidity Range
	50% ~ 98% RH

	
	 Humidity Deviation
	± 5% RH

	
	Water Spray Cycle
	1~9999H59M  (Adjustable)

	Constructure
	Controller
	Programmable color LCD touch screen controller

	
	Water supply system
	Automatic water supply

	
	
	Water purification system

	
	Build-in Water Tank(mm)
	270*300*900

	
	View Window Size(mm)
	250*330

	
	Air Circulation
	Centrifugal wind fan

	
	Radiometer
	UV Radiometer, Tolerance: ±5%

	
	Heating Element
	Nichrome heater

	
	Cooling System
	Mechanical compression refrigeration system

	
	Refrigerating Unit
	French TECUMSEH compressor

	
	Humidification System
	External isolation, stainless steel surface evaporation humidifier

	
	Air Circulation
	Centrifugal wind fan

	
	Safety Device
	 Over-temperature Protection; Over-current Protection; 

Water Shortage Protection; Earth leakage Protection; Phase Sequence Protection

	Material
	Exterior Material
	Steel plate with protective coating

	
	Interior Material
	SUS304 stainless steel

	
	Thermal Insulation
	Polyurethane foam and insulation cotton

	
	Observation Window
	Interior lighting, double-layer thermo stability silicone rubber sealing

	Power Supply
	AC380V 50Hz

	Maximum Noise

	65 dBA

	Environmental Conditional
	5℃～+35 ℃   ≤85% RH
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At present 7 Tier-one agents around the world provide LIB products, installation and maintenance service for customers. Make things simple and convenient.  
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XI'AN LIB ENVIRONMENTAL SIMULATION INDUSTRY


Climatic Test Chamber Manufacturer and Supplier 








Xenon Arc Weathering Test Chamber  


                                                


                                                 








Structures





Temperature & Humidity Test Chamber





Textile





Plastic





Paintings &coatings








Temperature Range


Ambient～100℃±2℃





Humidity Range


50%~98% RH





Irradiance


35~150 W/㎡





BPT 


35℃～85℃±2℃














XL-S-750





Xenon Arc Test Chamber





【Technical Parameter】








Standard: AATCC TM16,AATCC TM169,ASTM C1257,ASTM C1442,ASTM C1519,ASTM C732,ASTM C734,ASTM C793,ASTM D1148,ASTM D1670,ASTM D2565,ASTM D3424,ASTM D3451,ASTM D4101,ASTM D4303,ASTM D4355,ASTM D4434,ASTM D4459,ASTM D4798,ASTM D4811,ASTM D5019,ASTM D5071,ASTM D5383,ASTM D5398,ASTM D5819,ASTM D6083,ASTM D6551,ASTM D6577,ASTM D6662,ASTM D6695,ASTM D6878,ASTM D7356,ASTM D750,ASTM D7869,ASTM D882,ASTM D904,ASTM D925,ASTM F1164,ASTM F1515,ASTM F2366,ASTM G151,ASTM G155,GM 9125P,ISO 105-B07/B10,ISO 11341,ISO 12040,ISO 29664,ISO 4892-1 ,ISO 4892-2 ,SAE J2412,SAE J2527,VW PV 1306,VW PV 3929,VW PV 3930





* It's the fourth-generation upgraded xenon test chamber.





The controller is diversity designed,It can communication with LAN network interface by R-232 /R-485interface.


* pay attention to the environmental condition during installing








It can cool down to -86℃.


The Refrigerant can be replaced by R449A/R508B for Europe market.


The heat load can Absorbs 1000w in -20℃.














Structures





Xenon Arc Test Chamber





Appearance
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Safety protect system








Over Temperature Protection


Water Shortage Protection


Over Current Protection


Earth Leakage Protection


Phase Sequence Protection
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1.Workroom








The internal material is 304 stainless steel, mirror surface, rust-proof to high and low temperature and moisture corrosion resistance.


Nice ruggedness and long life.





7.Automatic Water Inlet 








Automatic control of the water intake of equipment, the customer can be directly connected to the laboratory faucet, so as to achieve automated testing;


Automatic inlet diameter 1/2 inch (13.5mm);


High and low water level alarm, water shortage lights and sound.


Standard 2 meter drain pipe.








4.Viewing Window 








Double layer insulating glass 8cm thickness, made of tempered glass.


The conductive film is located on the interior glass to prevent window frosting, built-in LED light for the work room lighting ;can clearly observe samples.


The light control button is located below the controller.

















2.Rotating Specimen Holder








8.Castor  








Install 4 castors for ease moving, and with brakes function. Caster height adjustable.








5.Controller  








PID programmable color touch screen controller, network connection computer.


Can edit 120 programs 100 segments.


LIB also can preset program into the controller based on user testing requirements.


The set system language is English for standard.





















































ogram into the controller based on user testing requirements.


The set system language is English for standard.





Inside there is a rotating specimen holder, which rotates around the xenon lamp，so that the irradiance received by the specimen is relatively uniform during the test. Total can mount 42 pieces of specimen.





9.Insulation  








10cm thick polyurethane foam and insulation cotton;


Better insulation performance, degradation resistance, environmental protection, noise reduction.





6.Water Re-circulation





Water purifier: mainly purification from water source to water tank.


Water re-circulation system that reduced water use and a series of water pipes








3. Irradiation Source 








Irradiation Source with 1 piece of 4500 W water-cooled xenon lamp with inner quartz and outer borosilicate filter


Average Lamp Life is 1600 hours. 














10.External Materials 








A3 steel plate with galvanized coating;


Electrostatic treatment; High and low temperature corrosion resistance; High hardness, anti - impact


Very high safety factor;


Color can be customized.





Core Function 








Structures





Xenon Arc Test Chamber





Two independent water way systems, one water tank supplies water to the lamp cooling and humidification system, and the other water tank supplies water to the water spray.








Water Way System





The water spray pipe is equipped with three nozzles, the diameter of the nozzle is 0.5mm, the settlement is 0.8 ~ 1.0mm / 80cm2 / H, and the flow rate is 0.3L / min, which simulates the outdoor moisture damage to the material.


Can be customized to front and rear spraying.








Water Spray System











Cooling System











After the liquid refrigerant absorbs the heat of the cooled object in the evaporator, it is vaporized into low-temperature and low-pressure steam, sucked by the compressor, compressed into high-pressure high-temperature steam, discharged into the condenser, and radiated to the cooling medium in the condenser, condensed into a high-pressure liquid, throttling through a throttle valve into a low-pressure low-temperature refrigerant, and again entering the evaporator to absorb heat and vaporize, to achieve the purpose of cycle refrigeration.


In this way, the refrigerant completes a refrigeration cycle through four basic processes of evaporation, compression, condensation, and throttling in the system.








UV Irradiance Radiometer is available for xenon test chamber.


The radiometer is a photoelectric sensor with fast response, reliable performance and high accuracy.








Radiometer





The blackboard thermometer is composed of a stainless steel flat plate with a length of 150 mm, a width of 70 mm, and a thickness of 1 mm. The side of the board facing the light source should be coated with a black flat lacquer to absorb at least 90% of the total incidence. The temperature measurement of the blackboard is made by a platinum resistance sensor located in the center of the plate.





Black Panel Thermometer











Protection System











Over Temperature Protection


Water Shortage Protection








Over Current Protection


Earth Leakage Protection


Phase Sequence Protection








Humidifier Dry Combustion Protection


Refrigerant High Pressure Protection








Option





Xenon Arc Test Chamber





Specimen Holder





Special specimen holder can be customized





Radiometer 





Demineralized Water 


Device





Reverse Osmosis Unit














WiFi connection


Mobile APP control


Multi-language controller interface：Russian,


French, Polish, Romanian, German

















Controller





Shipping & Packaging





Install Condition





      Environment Conditions


Temperature: +5°C ~ +35°C


Relative humidity: ≤85%;


Pressure: 86 KPa—106 KPa








Space Conditions


Sufficient space for ventilation








*Safety Instruction：1.Prohibited to test explosive, inflammable and high corrosive substance�2.Chemical exposure to the equipment is prohibited�3.Equipment must be safety on the ground to avoid electrostatic induction








Packaging











Plywood: standard wood export packaging.


The wooden box is fixed by sheet metal to 


prevent damage during transportation.





Gross weight: 500kgs~	


Package size: 1240*1160*2000 mm








First, seal chamber with waterproof plastic film.


Protect chamber from seawater corrosion.


Second, buffer foam is placed in the four 


corners of the chamber.It is used for fixing


equipment to prevent shaking and damaging 


chamber during transportation.








Shipping








+ 





Material：Export standard wooden box 


*Can be used for Sea, Air, Railway, Truck and


 multimodal transport.








Warranty & Service 


- 3 Years Warranty, Lifelong Follow-up Services





Professional After-sales Team


If you have any questions during operation,


we will supply solution to you with 24 hours.











Environment conditions


Temperature: +5°C ~ +35°C


Relative humidity: ≤85%;


Pressure: 86 KPa—106 KPa








How to Service





1. At first, our test chambers are produced based on 20 years product lifetime. 


Normally once test chambers have problems, we judge the problems, and send spare parts to our customers, and teach them how to change new parts on by email or video, all spare parts and shipping cost (by DHL, TNT, and FedEx) paid by LIB. 


2. If the customer needs our engineer on-site service, they only need pay the ticket accommodation to our Engineers, service is for free.


3. If products still can't use after our engineers repair, we will produce a new test chamber (same as the old one) to our customers with no charge. 














    Our company will repair the product, if the product, the material of the parts, the design and manufacturing of the products raised hardware problems caused by product itself rather than human error within three years warranty period since the date of dispatching by the customer. 


Our company repairs the products, but will collect the basic costs of the spare parts after the warranty period, but service is free always. 








Warranty Condition 








Xi’an LIB Environmental Simulation Industry








LIB Industry®








PROVIDING TEST SOLUTION, PROVIDING TEST EQUIPMENT








CE 


ROHS








Xi’an LIB Environmental Simulation Industry is a lead provider of environmental test chamber in China, with its own brand (LIB) design, production, sales and service since 2009. We continually update technology and develop new products for customer’s needs.


Our main products included temperature and climate test chambers, corrosion chambers, weathering testers, IP dust and rain chambers, ozone test chamber, noxious gas SO2 H2S chamber, walk-in chambers. We provide test chamber, we provide test solution. Standard and customized products to meet different customer needs.


By 2018, global market has spread to 53 countries to USA, Canada, Mexico, Brazil, Peru, Russia, German,UK,France,Finland,Netherlands, Poland,Switzerland,Thailand,Philippines, Singapore, Malaysia, Australian, South Africa etc. and the market continues to expand.
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LIB became a registered trademark of our company since 2017 year.





Contact Us


Website: www.lib-industry.com


Add: No.5 Zhangba First St, Xian High-Tech Area, Shaanxi ProvinceP.R.China  710065


Tel: +86 29 68918976  


WhatsApp: +86 18700875368 


Skype: serena_lib


Email: serena@ lib-industry.








Sales Team: � HYPERLINK "mailto:sales@lib-industry.com" �sales@lib-industry.com� 


After Sales Team：asd@lib-industry.com


Shipping Team：vip@lib-industry.com


Finance Team：account@lib-industry.com











